+-o HDEF@1F,3  <class IOPCIDevice, id 0x1000001f2, registered, matched, active, busy 0 (1684 ms), retain 10>
    {
      "assigned-addresses" = <10fb00827f000000000002a1000000000040000020fb00827f000000000000a10000000000000100>
      "MaximumBootBeepVolumeAlt" = <7f>
      "IOInterruptSpecifiers" = (<1000000007000000>,<0600000000000100>)
      "class-code" = <00030400>
      "IODeviceMemory" = (({"address"=548162109440,"length"=16384}),({"address"=548161978368,"length"=65536}))
      "IOReportLegendPublic" = Yes
      "MaximumBootBeepVolume" = <7f>
      "subsystem-vendor-id" = <aa170000>
      "PinConfigurations" = <1310210310011790f001f040301081034001a090>
      "acpi-device" = "IOACPIPlatformDevice is not serializable"
      "built-in" = <00>
      "IOPowerManagement" = {"ChildrenPowerState"=2,"CurrentPowerState"=2,"CapabilityFlags"=258,"ChildProxyPowerState"=2,"MaxPowerState"=3}
      "hda-gfx" = <"onboard-1">
      "IOInterruptControllers" = ("io-apic-0","IOPCIMessagedInterruptController")
      "IOPCIMSIMode" = Yes
      "vendor-id" = <86800000>
      "name" = <"pci8086,9d70">
      "device-id" = <709d0000>
      "alc-layout-id" = <0e000000>
      "layout-id" = <07000000>
      "acpi-pmcap-offset" = 80
      "compatible" = <"pci17aa,2238","pci8086,9d70","pciclass,040300","HDEF">
      "IOPCIResourced" = Yes
      "IOServiceDEXTEntitlements" = (("com.apple.developer.driverkit.transport.pci"))
      "AFGLowPowerState" = <03000000>
      "acpi-path" = "IOACPIPlane:/_SB/PCI0@0/HDEF@1f0003"
      "subsystem-id" = <38220000>
      "revision-id" = <21000000>
      "pcidebug" = "0:31:3"
      "IOName" = "pci8086,9d70"
      "IOReportLegend" = ({"IOReportGroupName"="Interrupt Statistics (by index)","IOReportChannels"=((5291294645182070784,4295098369,"               First Level Interrupt Handler Count"),(5291294645182070785,4295098369,"              Second Level Interrupt Handler Count"),(5291294645182070786,4295098369,"        First Level Interrupt Handler Time (MATUs)"),(5291294645182070787,4295098369,"   Second Level Interrupt Handler CPU Time (MATUs)"),(5291294645182070788,4295098369,"Second Level Interrupt Handler System Time (MATUs)")),"IOReportChannelInfo"={"IOReportChannelUnit"=0},"IOReportSubGroupName"="HDEF 1"})
      "reg" = <00fb00000000000000000000000000000000000010fb00020000000000000000000000000040000020fb000200000000000000000000000000000100>
    }
    

