Here are three circuits which are identical except for the frequency of the source. Inductors are able to "pass" lower frequencies more easily than higher ones, because they oppose changes in current, and low frequency AC has more gradual changes, giving the inductor a chance to adjust. The higher frequency of the bottom circuit results in a lower current.

Next: Impedances of Same Magnitude

Previous: Inductors of Various Inductances

Index

Simulator Home

java@falstad.com
Generated Wed Dec 7 2016